#
# I found this via searching the Intertubes, here:
# https://github.com/osmc/osmc/blob/master/package/remote-osmc/files/etc/lirc/apple-silver-A1294-lircd.conf
#
# See also: 
# https://github.com/osmc/osmc/blob/master/package/remote-osmc/files/etc/lirc/apple-white-A1156-lircd.conf
#####
# Please make this file available to others
# by sending it to <lirc@bartelmus.de>
#
# this config file was automatically generated
# using lirc-0.9.0(default) on Tue Jun  2 22:56:05 2015
#
# contributed by DBMandrake
#
# brand:                       Apple
# model no. of remote control: A1294 (silver)
# devices being controlled by this remote:
#

begin remote

  name  Apple_A1294
  bits            8
  flags SPACE_ENC|CONST_LENGTH
  eps            30
  aeps          100

  header       9140  4510
  one           633  1666
  zero          633   537
  ptrail        631
  repeat       9137  2220
  pre_data_bits   16
  pre_data       0x77E1
  post_data_bits  8
  post_data      0x2C
  gap          108756
  toggle_bit_mask 0x0
  ignore_mask 0x80ff

      begin codes
          KEY_UP                   0x50
          KEY_DOWN                 0x30
          KEY_LEFT                 0x90
          KEY_RIGHT                0x60
          KEY_OK                   0x3A 0xA0
          KEY_ESC                  0xC0
          KEY_PLAY                 0xFA 0xA0
      end codes

end remote